### Navigation

- index
- next |
- previous |
- OpenCV 3.0.0-dev documentation »
- OpenCV API Reference »
- imgproc. Image Processing »

# Motion Analysis and Object Tracking

## accumulate

Adds an image to the accumulator.

C++:`` void `accumulate`(InputArray src, InputOutputArray dst, InputArray mask=noArray() )

Python:`` `cv2.``accumulate`(src, dst[, mask]) → dst

C:`` void `cvAcc`(const CvArr* image, CvArr* sum, const CvArr* mask=NULL )

  Parameters: | src – Input image as 1- or 3-channel, 8-bit or 32-bit floating point. dst – Accumulator image with the same number of channels as input image, 32-bit or 64-bit floating-point. mask – Optional operation mask.

The function adds `src` or some of its elements to `dst` :

The function supports multi-channel images. Each channel is processed independently.

The functions `accumulate*` can be used, for example, to collect statistics of a scene background viewed by a still camera and for the further foreground-background segmentation.

See also

`accumulateSquare()`, `accumulateProduct()`, `accumulateWeighted()`

## accumulateSquare

Adds the square of a source image to the accumulator.

C++:`` void `accumulateSquare`(InputArray src, InputOutputArray dst, InputArray mask=noArray() )

Python:`` `cv2.``accumulateSquare`(src, dst[, mask]) → dst

C:`` void `cvSquareAcc`(const CvArr* image, CvArr* sqsum, const CvArr* mask=NULL )

  Parameters: | src – Input image as 1- or 3-channel, 8-bit or 32-bit floating point. dst – Accumulator image with the same number of channels as input image, 32-bit or 64-bit floating-point. mask – Optional operation mask.

The function adds the input image `src` or its selected region, raised to a power of 2, to the accumulator `dst` :

The function supports multi-channel images. Each channel is processed independently.

See also

`accumulateSquare()`, `accumulateProduct()`, `accumulateWeighted()`

## accumulateProduct

Adds the per-element product of two input images to the accumulator.

C++:`` void `accumulateProduct`(InputArray src1, InputArray src2, InputOutputArray dst, InputArray mask=noArray() )

Python:`` `cv2.``accumulateProduct`(src1, src2, dst[, mask]) → dst

C:`` void `cvMultiplyAcc`(const CvArr* image1, const CvArr* image2, CvArr* acc, const CvArr* mask=NULL )

  Parameters: | src1 – First input image, 1- or 3-channel, 8-bit or 32-bit floating point. src2 – Second input image of the same type and the same size as `src1` . dst – Accumulator with the same number of channels as input images, 32-bit or 64-bit floating-point. mask – Optional operation mask.

The function adds the product of two images or their selected regions to the accumulator `dst` :

The function supports multi-channel images. Each channel is processed independently.

See also

`accumulate()`, `accumulateSquare()`, `accumulateWeighted()`

## accumulateWeighted

Updates a running average.

C++:`` void `accumulateWeighted`(InputArray src, InputOutputArray dst, double alpha, InputArray mask=noArray() )

Python:`` `cv2.``accumulateWeighted`(src, dst, alpha[, mask]) → dst

C:`` void `cvRunningAvg`(const CvArr* image, CvArr* acc, double alpha, const CvArr* mask=NULL )

  Parameters: | src – Input image as 1- or 3-channel, 8-bit or 32-bit floating point. dst – Accumulator image with the same number of channels as input image, 32-bit or 64-bit floating-point. alpha – Weight of the input image. mask – Optional operation mask.

The function calculates the weighted sum of the input image `src` and the accumulator `dst` so that `dst` becomes a running average of a frame sequence:

That is, `alpha` regulates the update speed (how fast the accumulator “forgets” about earlier images). The function supports multi-channel images. Each channel is processed independently.

See also

`accumulate()`, `accumulateSquare()`, `accumulateProduct()`

## phaseCorrelate

The function is used to detect translational shifts that occur between two images. The operation takes advantage of the Fourier shift theorem for detecting the translational shift in the frequency domain. It can be used for fast image registration as well as motion estimation. For more information please see http://en.wikipedia.org/wiki/Phase_correlation .

Calculates the cross-power spectrum of two supplied source arrays. The arrays are padded if needed with `getOptimalDFTSize()`.

C++:`` Point2d `phaseCorrelate`(InputArray src1, InputArray src2, InputArray window=noArray(), double* response=0)

  Parameters: | src1 – Source floating point array (CV_32FC1 or CV_64FC1) src2 – Source floating point array (CV_32FC1 or CV_64FC1) window – Floating point array with windowing coefficients to reduce edge effects (optional). response – Signal power within the 5x5 centroid around the peak, between 0 and 1 (optional).

Return value: detected phase shift (sub-pixel) between the two arrays.

The function performs the following equations

- First it applies a Hanning window (see http://en.wikipedia.org/wiki/Hann_function) to each image to remove possible edge effects. This window is cached until the array size changes to speed up processing time.

- Next it computes the forward DFTs of each source array:

  where is the forward DFT.

- It then computes the cross-power spectrum of each frequency domain array:

- Next the cross-correlation is converted back into the time domain via the inverse DFT:

- Finally, it computes the peak location and computes a 5x5 weighted centroid around the peak to achieve sub-pixel accuracy.

- If non-zero, the response parameter is computed as the sum of the elements of r within the 5x5 centroid around the peak location. It is normalized to a maximum of 1 (meaning there is a single peak) and will be smaller when there are multiple peaks.

See also

`dft()`, `getOptimalDFTSize()`, `idft()`, `mulSpectrums()` `createHanningWindow()`

## createHanningWindow

This function computes a Hanning window coefficients in two dimensions. See http://en.wikipedia.org/wiki/Hann_function and http://en.wikipedia.org/wiki/Window_function for more information.

C++:`` void `createHanningWindow`(OutputArray dst, Size winSize, int type)

  Parameters: | dst – Destination array to place Hann coefficients in winSize – The window size specifications type – Created array type

An example is shown below:

    // create hanning window of size 100x100 and type CV_32F
    Mat hann;
    createHanningWindow(hann, Size(100, 100), CV_32F);

See also

`phaseCorrelate()`

## Help and Feedback

You did not find what you were looking for?

- Ask a question on the Q&A forum.
- If you think something is missing or wrong in the documentation, please file a bug report.

### Navigation

- index
- next |
- previous |
- OpenCV 3.0.0-dev documentation »
- OpenCV API Reference »
- imgproc. Image Processing »