### Navigation

- index
- next |
- previous |
- OpenCV 3.0.0-dev documentation »
- OpenCV API Reference »
- imgproc. Image Processing »

# Feature Detection

## Canny

Finds edges in an image using the [Canny86] algorithm.

C++:`` void `Canny`(InputArray image, OutputArray edges, double threshold1, double threshold2, int apertureSize=3, bool L2gradient=false )

Python:`` `cv2.``Canny`(image, threshold1, threshold2[, edges[, apertureSize[, L2gradient]]]) → edges

C:`` void `cvCanny`(const CvArr* image, CvArr* edges, double threshold1, double threshold2, int aperture_size=3 )

  Parameters: | image – 8-bit input image. edges – output edge map; single channels 8-bit image, which has the same size as `image` . threshold1 – first threshold for the hysteresis procedure. threshold2 – second threshold for the hysteresis procedure. apertureSize – aperture size for the `Sobel()` operator. L2gradient – a flag, indicating whether a more accurate norm should be used to calculate the image gradient magnitude ( `L2gradient=true` ), or whether the default norm is enough ( `L2gradient=false` ).

The function finds edges in the input image `image` and marks them in the output map `edges` using the Canny algorithm. The smallest value between `threshold1` and `threshold2` is used for edge linking. The largest value is used to find initial segments of strong edges. See http://en.wikipedia.org/wiki/Canny_edge_detector

Note

- An example on using the canny edge detector can be found at opencv_source_code/samples/cpp/edge.cpp
- (Python) An example on using the canny edge detector can be found at opencv_source_code/samples/python/edge.py

## cornerEigenValsAndVecs

Calculates eigenvalues and eigenvectors of image blocks for corner detection.

C++:`` void `cornerEigenValsAndVecs`(InputArray src, OutputArray dst, int blockSize, int ksize, int borderType=BORDER_DEFAULT )

Python:`` `cv2.``cornerEigenValsAndVecs`(src, blockSize, ksize[, dst[, borderType]]) → dst

C:`` void `cvCornerEigenValsAndVecs`(const CvArr* image, CvArr* eigenvv, int block_size, int aperture_size=3 )

  Parameters: | src – Input single-channel 8-bit or floating-point image. dst – Image to store the results. It has the same size as `src` and the type `CV_32FC(6)` . blockSize – Neighborhood size (see details below). ksize – Aperture parameter for the `Sobel()` operator. borderType – Pixel extrapolation method. See `borderInterpolate()` .

For every pixel , the function `cornerEigenValsAndVecs` considers a `blockSize` `blockSize` neighborhood . It calculates the covariation matrix of derivatives over the neighborhood as:

where the derivatives are computed using the `Sobel()` operator.

After that, it finds eigenvectors and eigenvalues of and stores them in the destination image as where

- are the non-sorted eigenvalues of
- are the eigenvectors corresponding to
- are the eigenvectors corresponding to

The output of the function can be used for robust edge or corner detection.

See also

`cornerMinEigenVal()`, `cornerHarris()`, `preCornerDetect()`

Note

- (Python) An example on how to use eigenvectors and eigenvalues to estimate image texture flow direction can be found at opencv_source_code/samples/python2/texture_flow.py

## cornerHarris

Harris corner detector.

C++:`` void `cornerHarris`(InputArray src, OutputArray dst, int blockSize, int ksize, double k, int borderType=BORDER_DEFAULT )

Python:`` `cv2.``cornerHarris`(src, blockSize, ksize, k[, dst[, borderType]]) → dst

C:`` void `cvCornerHarris`(const CvArr* image, CvArr* harris_response, int block_size, int aperture_size=3, double k=0.04 )

  Parameters: | src – Input single-channel 8-bit or floating-point image. dst – Image to store the Harris detector responses. It has the type `CV_32FC1` and the same size as `src` . blockSize – Neighborhood size (see the details on `cornerEigenValsAndVecs()` ). ksize – Aperture parameter for the `Sobel()` operator. k – Harris detector free parameter. See the formula below. borderType – Pixel extrapolation method. See `borderInterpolate()` .

The function runs the Harris corner detector on the image. Similarly to `cornerMinEigenVal()` and `cornerEigenValsAndVecs()` , for each pixel it calculates a gradient covariance matrix over a neighborhood. Then, it computes the following characteristic:

Corners in the image can be found as the local maxima of this response map.

## cornerMinEigenVal

Calculates the minimal eigenvalue of gradient matrices for corner detection.

C++:`` void `cornerMinEigenVal`(InputArray src, OutputArray dst, int blockSize, int ksize=3, int borderType=BORDER_DEFAULT )

Python:`` `cv2.``cornerMinEigenVal`(src, blockSize[, dst[, ksize[, borderType]]]) → dst

C:`` void `cvCornerMinEigenVal`(const CvArr* image, CvArr* eigenval, int block_size, int aperture_size=3 )

  Parameters: | src – Input single-channel 8-bit or floating-point image. dst – Image to store the minimal eigenvalues. It has the type `CV_32FC1` and the same size as `src` . blockSize – Neighborhood size (see the details on `cornerEigenValsAndVecs()` ). ksize – Aperture parameter for the `Sobel()` operator. borderType – Pixel extrapolation method. See `borderInterpolate()` .

The function is similar to `cornerEigenValsAndVecs()` but it calculates and stores only the minimal eigenvalue of the covariance matrix of derivatives, that is, in terms of the formulae in the `cornerEigenValsAndVecs()` description.

## cornerSubPix

Refines the corner locations.

C++:`` void `cornerSubPix`(InputArray image, InputOutputArray corners, Size winSize, Size zeroZone, TermCriteria criteria)

Python:`` `cv2.``cornerSubPix`(image, corners, winSize, zeroZone, criteria) → corners

C:`` void `cvFindCornerSubPix`(const CvArr* image, CvPoint2D32f* corners, int count, CvSize win, CvSize zero_zone, CvTermCriteria criteria)

  Parameters: | image – Input image. corners – Initial coordinates of the input corners and refined coordinates provided for output. winSize – Half of the side length of the search window. For example, if `winSize=Size(5,5)` , then a search window is used. zeroZone – Half of the size of the dead region in the middle of the search zone over which the summation in the formula below is not done. It is used sometimes to avoid possible singularities of the autocorrelation matrix. The value of (-1,-1) indicates that there is no such a size. criteria – Criteria for termination of the iterative process of corner refinement. That is, the process of corner position refinement stops either after `criteria.maxCount` iterations or when the corner position moves by less than `criteria.epsilon` on some iteration.

The function iterates to find the sub-pixel accurate location of corners or radial saddle points, as shown on the figure below.

Sub-pixel accurate corner locator is based on the observation that every vector from the center to a point located within a neighborhood of is orthogonal to the image gradient at subject to image and measurement noise. Consider the expression:

where is an image gradient at one of the points in a neighborhood of . The value of is to be found so that is minimized. A system of equations may be set up with set to zero:

where the gradients are summed within a neighborhood (“search window”) of . Calling the first gradient term and the second gradient term gives:

The algorithm sets the center of the neighborhood window at this new center and then iterates until the center stays within a set threshold.

## goodFeaturesToTrack

Determines strong corners on an image.

C++:`` void `goodFeaturesToTrack`(InputArray image, OutputArray corners, int maxCorners, double qualityLevel, double minDistance, InputArray mask=noArray(), int blockSize=3, bool useHarrisDetector=false, double k=0.04 )

Python:`` `cv2.``goodFeaturesToTrack`(image, maxCorners, qualityLevel, minDistance[, corners[, mask[, blockSize[, useHarrisDetector[, k]]]]]) → corners

C:`` void `cvGoodFeaturesToTrack`(const CvArr* image, CvArr* eig_image, CvArr* temp_image, CvPoint2D32f* corners, int* corner_count, double quality_level, double min_distance, const CvArr* mask=NULL, int block_size=3, int use_harris=0, double k=0.04 )

  Parameters: | image – Input 8-bit or floating-point 32-bit, single-channel image. eig_image – The parameter is ignored. temp_image – The parameter is ignored. corners – Output vector of detected corners. maxCorners – Maximum number of corners to return. If there are more corners than are found, the strongest of them is returned. qualityLevel – Parameter characterizing the minimal accepted quality of image corners. The parameter value is multiplied by the best corner quality measure, which is the minimal eigenvalue (see `cornerMinEigenVal()` ) or the Harris function response (see `cornerHarris()` ). The corners with the quality measure less than the product are rejected. For example, if the best corner has the quality measure = 1500, and the `qualityLevel=0.01` , then all the corners with the quality measure less than 15 are rejected. minDistance – Minimum possible Euclidean distance between the returned corners. mask – Optional region of interest. If the image is not empty (it needs to have the type `CV_8UC1` and the same size as `image` ), it specifies the region in which the corners are detected. blockSize – Size of an average block for computing a derivative covariation matrix over each pixel neighborhood. See `cornerEigenValsAndVecs()` . useHarrisDetector – Parameter indicating whether to use a Harris detector (see `cornerHarris()`) or `cornerMinEigenVal()`. k – Free parameter of the Harris detector.

The function finds the most prominent corners in the image or in the specified image region, as described in [Shi94]:

1. Function calculates the corner quality measure at every source image pixel using the `cornerMinEigenVal()` or `cornerHarris()` .
2. Function performs a non-maximum suppression (the local maximums in 3 x 3 neighborhood are retained).
3. The corners with the minimal eigenvalue less than are rejected.
4. The remaining corners are sorted by the quality measure in the descending order.
5. Function throws away each corner for which there is a stronger corner at a distance less than `maxDistance`.

The function can be used to initialize a point-based tracker of an object.

Note

If the function is called with different values `A` and `B` of the parameter `qualityLevel` , and `A` > {B}, the vector of returned corners with `qualityLevel=A` will be the prefix of the output vector with `qualityLevel=B` .

See also

`cornerMinEigenVal()`, `cornerHarris()`, `calcOpticalFlowPyrLK()`, `estimateRigidTransform()`,

## HoughCircles

Finds circles in a grayscale image using the Hough transform.

C++:`` void `HoughCircles`(InputArray image, OutputArray circles, int method, double dp, double minDist, double param1=100, double param2=100, int minRadius=0, int maxRadius=0 )

C:`` CvSeq* `cvHoughCircles`(CvArr* image, void* circle_storage, int method, double dp, double min_dist, double param1=100, double param2=100, int min_radius=0, int max_radius=0 )

Python:`` `cv2.``HoughCircles`(image, method, dp, minDist[, circles[, param1[, param2[, minRadius[, maxRadius]]]]]) → circles

  Parameters: | image – 8-bit, single-channel, grayscale input image. circles – Output vector of found circles. Each vector is encoded as a 3-element floating-point vector . circle_storage – In C function this is a memory storage that will contain the output sequence of found circles. method – Detection method to use. Currently, the only implemented method is `CV_HOUGH_GRADIENT` , which is basically 21HT , described in [Yuen90]. dp – Inverse ratio of the accumulator resolution to the image resolution. For example, if `dp=1` , the accumulator has the same resolution as the input image. If `dp=2` , the accumulator has half as big width and height. minDist – Minimum distance between the centers of the detected circles. If the parameter is too small, multiple neighbor circles may be falsely detected in addition to a true one. If it is too large, some circles may be missed. param1 – First method-specific parameter. In case of `CV_HOUGH_GRADIENT` , it is the higher threshold of the two passed to the `Canny()` edge detector (the lower one is twice smaller). param2 – Second method-specific parameter. In case of `CV_HOUGH_GRADIENT` , it is the accumulator threshold for the circle centers at the detection stage. The smaller it is, the more false circles may be detected. Circles, corresponding to the larger accumulator values, will be returned first. minRadius – Minimum circle radius. maxRadius – Maximum circle radius.

The function finds circles in a grayscale image using a modification of the Hough transform.

Example:

    #include <opencv2/imgproc.hpp>
    #include <opencv2/highgui.hpp>
    #include <math.h>

    using namespace cv;

    int main(int argc, char** argv)
    {
        Mat img, gray;
        if( argc != 2 && !(img=imread(argv[1], 1)).data)
            return -1;
        cvtColor(img, gray, COLOR_BGR2GRAY);
        // smooth it, otherwise a lot of false circles may be detected
        GaussianBlur( gray, gray, Size(9, 9), 2, 2 );
        vector<Vec3f> circles;
        HoughCircles(gray, circles, HOUGH_GRADIENT,
                     2, gray->rows/4, 200, 100 );
        for( size_t i = 0; i < circles.size(); i++ )
        {
             Point center(cvRound(circles[i][0]), cvRound(circles[i][1]));
             int radius = cvRound(circles[i][2]);
             // draw the circle center
             circle( img, center, 3, Scalar(0,255,0), -1, 8, 0 );
             // draw the circle outline
             circle( img, center, radius, Scalar(0,0,255), 3, 8, 0 );
        }
        namedWindow( "circles", 1 );
        imshow( "circles", img );
        return 0;
    }

Note

Usually the function detects the centers of circles well. However, it may fail to find correct radii. You can assist to the function by specifying the radius range ( `minRadius` and `maxRadius` ) if you know it. Or, you may ignore the returned radius, use only the center, and find the correct radius using an additional procedure.

See also

`fitEllipse()`, `minEnclosingCircle()`

Note

- An example using the Hough circle detector can be found at opencv_source_code/samples/cpp/houghcircles.cpp

## HoughLines

Finds lines in a binary image using the standard Hough transform.

C++:`` void `HoughLines`(InputArray image, OutputArray lines, double rho, double theta, int threshold, double srn=0, double stn=0, double min_theta=0, double max_theta=CV_PI )

Python:`` `cv2.``HoughLines`(image, rho, theta, threshold[, lines[, srn[, stn[, min_theta[, max_theta]]]]]) → lines

C:`` CvSeq* `cvHoughLines2`(CvArr* image, void* line_storage, int method, double rho, double theta, int threshold, double param1=0, double param2=0, double min_theta=0, double max_theta=CV_PI )

  Parameters: | image – 8-bit, single-channel binary source image. The image may be modified by the function. lines – Output vector of lines. Each line is represented by a two-element vector . is the distance from the coordinate origin (top-left corner of the image). is the line rotation angle in radians ( ). rho – Distance resolution of the accumulator in pixels. theta – Angle resolution of the accumulator in radians. threshold – Accumulator threshold parameter. Only those lines are returned that get enough votes ( ). srn – For the multi-scale Hough transform, it is a divisor for the distance resolution `rho` . The coarse accumulator distance resolution is `rho` and the accurate accumulator resolution is `rho/srn` . If both `srn=0` and `stn=0` , the classical Hough transform is used. Otherwise, both these parameters should be positive. stn – For the multi-scale Hough transform, it is a divisor for the distance resolution `theta`. min_theta – For standard and multi-scale Hough transform, minimum angle to check for lines. Must fall between 0 and max_theta. max_theta – For standard and multi-scale Hough transform, maximum angle to check for lines. Must fall between min_theta and CV_PI. method – One of the following Hough transform variants: CV_HOUGH_STANDARD classical or standard Hough transform. Every line is represented by two floating-point numbers , where is a distance between (0,0) point and the line, and is the angle between x-axis and the normal to the line. Thus, the matrix must be (the created sequence will be) of `CV_32FC2` type CV_HOUGH_PROBABILISTIC probabilistic Hough transform (more efficient in case if the picture contains a few long linear segments). It returns line segments rather than the whole line. Each segment is represented by starting and ending points, and the matrix must be (the created sequence will be) of the `CV_32SC4` type. CV_HOUGH_MULTI_SCALE multi-scale variant of the classical Hough transform. The lines are encoded the same way as `CV_HOUGH_STANDARD`. param1 – First method-dependent parameter: For the classical Hough transform, it is not used (0). For the probabilistic Hough transform, it is the minimum line length. For the multi-scale Hough transform, it is `srn`. param2 – Second method-dependent parameter: For the classical Hough transform, it is not used (0). For the probabilistic Hough transform, it is the maximum gap between line segments lying on the same line to treat them as a single line segment (that is, to join them). For the multi-scale Hough transform, it is `stn`.

The function implements the standard or standard multi-scale Hough transform algorithm for line detection. See http://homepages.inf.ed.ac.uk/rbf/HIPR2/hough.htm for a good explanation of Hough transform. See also the example in `HoughLinesP()` description.

Note

- An example using the Hough line detector can be found at opencv_source_code/samples/cpp/houghlines.cpp

## HoughLinesP

Finds line segments in a binary image using the probabilistic Hough transform.

C++:`` void `HoughLinesP`(InputArray image, OutputArray lines, double rho, double theta, int threshold, double minLineLength=0, double maxLineGap=0 )

Python:`` `cv2.``HoughLinesP`(image, rho, theta, threshold[, lines[, minLineLength[, maxLineGap]]]) → lines

  Parameters: | image – 8-bit, single-channel binary source image. The image may be modified by the function. lines – Output vector of lines. Each line is represented by a 4-element vector , where and are the ending points of each detected line segment. rho – Distance resolution of the accumulator in pixels. theta – Angle resolution of the accumulator in radians. threshold – Accumulator threshold parameter. Only those lines are returned that get enough votes ( ). minLineLength – Minimum line length. Line segments shorter than that are rejected. maxLineGap – Maximum allowed gap between points on the same line to link them.

The function implements the probabilistic Hough transform algorithm for line detection, described in [Matas00]. See the line detection example below:

    /* This is a standalone program. Pass an image name as the first parameter
    of the program.  Switch between standard and probabilistic Hough transform
    by changing "#if 1" to "#if 0" and back */
    #include <opencv2/imgproc.hpp>
    #include <opencv2/highgui.hpp>

    using namespace cv;

    int main(int argc, char** argv)
    {
        Mat src, dst, color_dst;
        if( argc != 2 || !(src=imread(argv[1], 0)).data)
            return -1;

        Canny( src, dst, 50, 200, 3 );
        cvtColor( dst, color_dst, COLOR_GRAY2BGR );

    #if 0
        vector<Vec2f> lines;
        HoughLines( dst, lines, 1, CV_PI/180, 100 );

        for( size_t i = 0; i < lines.size(); i++ )
        {
            float rho = lines[i][0];
            float theta = lines[i][1];
            double a = cos(theta), b = sin(theta);
            double x0 = a*rho, y0 = b*rho;
            Point pt1(cvRound(x0 + 1000*(-b)),
                      cvRound(y0 + 1000*(a)));
            Point pt2(cvRound(x0 - 1000*(-b)),
                      cvRound(y0 - 1000*(a)));
            line( color_dst, pt1, pt2, Scalar(0,0,255), 3, 8 );
        }
    #else
        vector<Vec4i> lines;
        HoughLinesP( dst, lines, 1, CV_PI/180, 80, 30, 10 );
        for( size_t i = 0; i < lines.size(); i++ )
        {
            line( color_dst, Point(lines[i][0], lines[i][1]),
                Point(lines[i][2], lines[i][3]), Scalar(0,0,255), 3, 8 );
        }
    #endif
        namedWindow( "Source", 1 );
        imshow( "Source", src );

        namedWindow( "Detected Lines", 1 );
        imshow( "Detected Lines", color_dst );

        waitKey(0);
        return 0;
    }

This is a sample picture the function parameters have been tuned for:

And this is the output of the above program in case of the probabilistic Hough transform:

See also

`LineSegmentDetector`

## LineSegmentDetector

Line segment detector class, following the algorithm described at [Rafael12].

class `LineSegmentDetector` : public `Algorithm`

## createLineSegmentDetector

Creates a smart pointer to a LineSegmentDetector object and initializes it.

C++:`` Ptr<LineSegmentDetector> `createLineSegmentDetector`(int _refine=LSD_REFINE_STD, double _scale=0.8, double _sigma_scale=0.6, double _quant=2.0, double _ang_th=22.5, double _log_eps=0, double _density_th=0.7, int _n_bins=1024)

Python:`` `cv2.``createLineSegmentDetector`([_refine[, _scale[, _sigma_scale[, _quant[, _ang_th[, _log_eps[, _density_th[, _n_bins]]]]]]]]) → retval

  Parameters: | _refine – The way found lines will be refined: LSD_REFINE_NONE - No refinement applied. LSD_REFINE_STD - Standard refinement is applied. E.g. breaking arches into smaller straighter line approximations. LSD_REFINE_ADV - Advanced refinement. Number of false alarms is calculated, lines are refined through increase of precision, decrement in size, etc. scale – The scale of the image that will be used to find the lines. Range (0..1]. sigma_scale – Sigma for Gaussian filter. It is computed as sigma = _sigma_scale/_scale. quant – Bound to the quantization error on the gradient norm. ang_th – Gradient angle tolerance in degrees. log_eps – Detection threshold: -log10(NFA) > log_eps. Used only when advancent refinement is chosen. density_th – Minimal density of aligned region points in the enclosing rectangle. n_bins – Number of bins in pseudo-ordering of gradient modulus.

The LineSegmentDetector algorithm is defined using the standard values. Only advanced users may want to edit those, as to tailor it for their own application.

## LineSegmentDetector::detect

Finds lines in the input image. See the lsd_lines.cpp sample for possible usage.

C++:`` void `LineSegmentDetector::``detect`(const InputArray _image, OutputArray _lines, OutputArray width=noArray(), OutputArray prec=noArray(), OutputArray nfa=noArray())

Python:`` `cv2.createLineSegmentDetector.``detect`(_image[, _lines[, width[, prec[, nfa]]]]) → _lines, width, prec, nfa
  :param _image A grayscale (CV_8UC1) input image.
    If only a roi needs to be selected, use :: lsd_ptr->detect(image(roi), lines, ...); lines += Scalar(roi.x, roi.y, roi.x, roi.y);

  Parameters: | lines – A vector of Vec4i elements specifying the beginning and ending point of a line. Where Vec4i is (x1, y1, x2, y2), point 1 is the start, point 2 - end. Returned lines are strictly oriented depending on the gradient. width – Vector of widths of the regions, where the lines are found. E.g. Width of line. prec – Vector of precisions with which the lines are found. nfa – Vector containing number of false alarms in the line region, with precision of 10%. The bigger the value, logarithmically better the detection. -1 corresponds to 10 mean false alarms 0 corresponds to 1 mean false alarm 1 corresponds to 0.1 mean false alarms

  This vector will be calculated only when the objects type is LSD_REFINE_ADV.

This is the output of the default parameters of the algorithm on the above shown image.

Note

- An example using the LineSegmentDetector can be found at opencv_source_code/samples/cpp/lsd_lines.cpp

## LineSegmentDetector::drawSegments

Draws the line segments on a given image.

C++:`` void `LineSegmentDetector::``drawSegments`(InputOutputArray _image, InputArray lines)

Python:`` `cv2.createLineSegmentDetector.``drawSegments`(_image, lines) → _image

  Parameters: | image – The image, where the liens will be drawn. Should be bigger or equal to the image, where the lines were found. lines – A vector of the lines that needed to be drawn.

## LineSegmentDetector::compareSegments

Draws two groups of lines in blue and red, counting the non overlapping (mismatching) pixels.

C++:`` int `LineSegmentDetector::``compareSegments`(const Size& size, InputArray lines1, InputArray lines2, InputOutputArray _image=noArray())

Python:`` `cv2.createLineSegmentDetector.``compareSegments`(size, lines1, lines2[, _image]) → retval, _image

  Parameters: | size – The size of the image, where lines1 and lines2 were found. lines1 – The first group of lines that needs to be drawn. It is visualized in blue color. lines2 – The second group of lines. They visualized in red color. image – Optional image, where the lines will be drawn. The image should be color(3-channel) in order for lines1 and lines2 to be drawn in the above mentioned colors.

## preCornerDetect

Calculates a feature map for corner detection.

C++:`` void `preCornerDetect`(InputArray src, OutputArray dst, int ksize, int borderType=BORDER_DEFAULT )

Python:`` `cv2.``preCornerDetect`(src, ksize[, dst[, borderType]]) → dst

C:`` void `cvPreCornerDetect`(const CvArr* image, CvArr* corners, int aperture_size=3 )

  Parameters: | src – Source single-channel 8-bit of floating-point image. dst – Output image that has the type `CV_32F` and the same size as `src` . ksize – Aperture size of the `Sobel()` . borderType – Pixel extrapolation method. See `borderInterpolate()` .

The function calculates the complex spatial derivative-based function of the source image

where ,:math:D_y are the first image derivatives, ,:math:D_{yy} are the second image derivatives, and is the mixed derivative.

The corners can be found as local maximums of the functions, as shown below:

    Mat corners, dilated_corners;
    preCornerDetect(image, corners, 3);
    // dilation with 3x3 rectangular structuring element
    dilate(corners, dilated_corners, Mat(), 1);
    Mat corner_mask = corners == dilated_corners;

[Canny86] | Canny. A Computational Approach to Edge Detection, IEEE Trans. on Pattern Analysis and Machine Intelligence, 8(6), pp. 679-698 (1986).

[Matas00] | Matas, J. and Galambos, C. and Kittler, J.V., Robust Detection of Lines Using the Progressive Probabilistic Hough Transform. CVIU 78 1, pp 119-137 (2000)

[Shi94] | Shi and C. Tomasi. Good Features to Track. Proceedings of the IEEE Conference on Computer Vision and Pattern Recognition, pages 593-600, June 1994.

[Yuen90] | Yuen, H. K. and Princen, J. and Illingworth, J. and Kittler, J., Comparative study of Hough transform methods for circle finding. Image Vision Comput. 8 1, pp 71–77 (1990)

[Rafael12] | Rafael Grompone von Gioi, Jérémie Jakubowicz, Jean-Michel Morel, and Gregory Randall, LSD: a Line Segment Detector, Image Processing On Line, vol. 2012. http://dx.doi.org/10.5201/ipol.2012.gjmr-lsd

## Help and Feedback

You did not find what you were looking for?

- Ask a question on the Q&A forum.
- If you think something is missing or wrong in the documentation, please file a bug report.

### Navigation

- index
- next |
- previous |
- OpenCV 3.0.0-dev documentation »
- OpenCV API Reference »
- imgproc. Image Processing »