| OpenCV 3.4.3 Open Source Computer Vision

Sobel Derivatives

Prev Tutorial: Adding borders to your images

Next Tutorial: Laplace Operator

## Goal

In this tutorial you will learn how to:

- Use the OpenCV function Sobel() to calculate the derivatives from an image.
- Use the OpenCV function Scharr() to calculate a more accurate derivative for a kernel of size \(3 \cdot 3\)

## Theory

Note
  The explanation below belongs to the book Learning OpenCV by Bradski and Kaehler.

1. In the last two tutorials we have seen applicative examples of convolutions. One of the most important convolutions is the computation of derivatives in an image (or an approximation to them).

2. Why may be important the calculus of the derivatives in an image? Let's imagine we want to detect the edges present in the image. For instance:

   You can easily notice that in an edge, the pixel intensity changes in a notorious way. A good way to express changes is by using derivatives. A high change in gradient indicates a major change in the image.

3. To be more graphical, let's assume we have a 1D-image. An edge is shown by the "jump" in intensity in the plot below:

4. The edge "jump" can be seen more easily if we take the first derivative (actually, here appears as a maximum)

5. So, from the explanation above, we can deduce that a method to detect edges in an image can be performed by locating pixel locations where the gradient is higher than its neighbors (or to generalize, higher than a threshold).
6. More detailed explanation, please refer to Learning OpenCV by Bradski and Kaehler

### Sobel Operator

1. The Sobel Operator is a discrete differentiation operator. It computes an approximation of the gradient of an image intensity function.
2. The Sobel Operator combines Gaussian smoothing and differentiation.

#### Formulation

Assuming that the image to be operated is \(I\):

1. We calculate two derivatives:

   1. Horizontal changes: This is computed by convolving \(I\) with a kernel \(G_{x}\) with odd size. For example for a kernel size of 3, \(G_{x}\) would be computed as:

   \[G_{x} = \begin{bmatrix} -1 & 0 & +1 \\ -2 & 0 & +2 \\ -1 & 0 & +1 \end{bmatrix} * I\]

   1. Vertical changes: This is computed by convolving \(I\) with a kernel \(G_{y}\) with odd size. For example for a kernel size of 3, \(G_{y}\) would be computed as:

   \[G_{y} = \begin{bmatrix} -1 & -2 & -1 \\ 0 & 0 & 0 \\ +1 & +2 & +1 \end{bmatrix} * I\]

2. At each point of the image we calculate an approximation of the gradient in that point by combining both results above:

   \[G = \sqrt{ G_{x}^{2} + G_{y}^{2} }\]

   Although sometimes the following simpler equation is used:

   \[G = |G_{x}| + |G_{y}|\]

Note
  When the size of the kernel is `3`, the Sobel kernel shown above may produce noticeable inaccuracies (after all, Sobel is only an approximation of the derivative). OpenCV addresses this inaccuracy for kernels of size 3 by using the Scharr() function. This is as fast but more accurate than the standard Sobel function. It implements the following kernels:

  \[G_{x} = \begin{bmatrix} -3 & 0 & +3 \\ -10 & 0 & +10 \\ -3 & 0 & +3 \end{bmatrix}\]

  \[G_{y} = \begin{bmatrix} -3 & -10 & -3 \\ 0 & 0 & 0 \\ +3 & +10 & +3 \end{bmatrix}\]

  You can check out more information of this function in the OpenCV reference - Scharr() . Also, in the sample code below, you will notice that above the code for Sobel() function there is also code for the Scharr() function commented. Uncommenting it (and obviously commenting the Sobel stuff) should give you an idea of how this function works.

## Code

1. What does this program do?
   - Applies the Sobel Operator and generates as output an image with the detected edges bright on a darker background.
2. The tutorial code's is shown lines below.

C++

You can also download it from here

#include "opencv2/imgproc.hpp"
#include "opencv2/imgcodecs.hpp"
#include "opencv2/highgui.hpp"
#include <iostream>
using namespace cv;
using namespace std;
int main( int argc, char** argv )
{
cv::CommandLineParser parser(argc, argv,
"{@input |../data/lena.jpg|input image}"
"{ksize k|1|ksize (hit 'K' to increase its value)}"
"{scale s|1|scale (hit 'S' to increase its value)}"
"{delta d|0|delta (hit 'D' to increase its value)}"
"{help h|false|show help message}");
cout << "The sample uses Sobel or Scharr OpenCV functions for edge detection\n\n";
parser.printMessage();
cout << "\nPress 'ESC' to exit program.\nPress 'R' to reset values ( ksize will be -1 equal to Scharr function )";
// First we declare the variables we are going to use
Mat image,src, src_gray;
Mat grad;
const String window_name = "Sobel Demo - Simple Edge Detector";
int ksize = parser.get<int>("ksize");
int scale = parser.get<int>("scale");
int delta = parser.get<int>("delta");
int ddepth = CV_16S;
String imageName = parser.get<String>("@input");
// As usual we load our source image (src)
image = imread( imageName, IMREAD_COLOR ); // Load an image
// Check if image is loaded fine
if( image.empty() )
{
printf("Error opening image: %s\n", imageName.c_str());
return 1;
}
for (;;)
{
// Remove noise by blurring with a Gaussian filter ( kernel size = 3 )
GaussianBlur(image, src, Size(3, 3), 0, 0, BORDER_DEFAULT);
// Convert the image to grayscale
cvtColor(src, src_gray, COLOR_BGR2GRAY);
Mat grad_x, grad_y;
Mat abs_grad_x, abs_grad_y;
Sobel(src_gray, grad_x, ddepth, 1, 0, ksize, scale, delta, BORDER_DEFAULT);
Sobel(src_gray, grad_y, ddepth, 0, 1, ksize, scale, delta, BORDER_DEFAULT);
// converting back to CV_8U
convertScaleAbs(grad_x, abs_grad_x);
convertScaleAbs(grad_y, abs_grad_y);
addWeighted(abs_grad_x, 0.5, abs_grad_y, 0.5, 0, grad);
imshow(window_name, grad);
char key = (char)waitKey(0);
if(key == 27)
{
return 0;
}
if (key == 'k' || key == 'K')
{
ksize = ksize < 30 ? ksize+2 : -1;
}
if (key == 's' || key == 'S')
{
scale++;
}
if (key == 'd' || key == 'D')
{
delta++;
}
if (key == 'r' || key == 'R')
{
scale = 1;
ksize = -1;
delta = 0;
}
}
return 0;
}
Java

You can also download it from here

import org.opencv.core.*;
import org.opencv.highgui.HighGui;
import org.opencv.imgcodecs.Imgcodecs;
import org.opencv.imgproc.Imgproc;
class SobelDemoRun {
public void run(String[] args) {
// First we declare the variables we are going to use
Mat src, src_gray = new Mat();
Mat grad = new Mat();
String window_name = "Sobel Demo - Simple Edge Detector";
int scale = 1;
int delta = 0;
int ddepth = CvType.CV_16S;
// As usual we load our source image (src)
// Check number of arguments
if (args.length == 0){
System.out.println("Not enough parameters!");
System.out.println("Program Arguments: [image_path]");
System.exit(-1);
}
// Load the image
src = Imgcodecs.imread(args[0]);
// Check if image is loaded fine
if( src.empty() ) {
System.out.println("Error opening image: " + args[0]);
System.exit(-1);
}
// Remove noise by blurring with a Gaussian filter ( kernel size = 3 )
Imgproc.GaussianBlur( src, src, new Size(3, 3), 0, 0, Core.BORDER_DEFAULT );
// Convert the image to grayscale
Imgproc.cvtColor( src, src_gray, Imgproc.COLOR_RGB2GRAY );
Mat grad_x = new Mat(), grad_y = new Mat();
Mat abs_grad_x = new Mat(), abs_grad_y = new Mat();
//Imgproc.Scharr( src_gray, grad_x, ddepth, 1, 0, scale, delta, Core.BORDER_DEFAULT );
Imgproc.Sobel( src_gray, grad_x, ddepth, 1, 0, 3, scale, delta, Core.BORDER_DEFAULT );
//Imgproc.Scharr( src_gray, grad_y, ddepth, 0, 1, scale, delta, Core.BORDER_DEFAULT );
Imgproc.Sobel( src_gray, grad_y, ddepth, 0, 1, 3, scale, delta, Core.BORDER_DEFAULT );
// converting back to CV_8U
Core.convertScaleAbs( grad_x, abs_grad_x );
Core.convertScaleAbs( grad_y, abs_grad_y );
Core.addWeighted( abs_grad_x, 0.5, abs_grad_y, 0.5, 0, grad );
HighGui.imshow( window_name, grad );
HighGui.waitKey(0);
System.exit(0);
}
}
public class SobelDemo {
public static void main(String[] args) {
// Load the native library.
System.loadLibrary(Core.NATIVE_LIBRARY_NAME);
new SobelDemoRun().run(args);
}
}
Python

You can also download it from here

"""
@file sobel_demo.py
@brief Sample code using Sobel and/or Scharr OpenCV functions to make a simple Edge Detector
"""
import sys
import cv2 as cv
def main(argv):
window_name = ('Sobel Demo - Simple Edge Detector')
scale = 1
delta = 0
ddepth = cv.CV_16S
if len(argv) < 1:
print ('Not enough parameters')
print ('Usage:\nmorph_lines_detection.py < path_to_image >')
return -1
# Load the image
src = cv.imread(argv[0], cv.IMREAD_COLOR)
# Check if image is loaded fine
if src is None:
print ('Error opening image: ' + argv[0])
return -1
src = cv.GaussianBlur(src, (3, 3), 0)
gray = cv.cvtColor(src, cv.COLOR_BGR2GRAY)
grad_x = cv.Sobel(gray, ddepth, 1, 0, ksize=3, scale=scale, delta=delta, borderType=cv.BORDER_DEFAULT)
# Gradient-Y
# grad_y = cv.Scharr(gray,ddepth,0,1)
grad_y = cv.Sobel(gray, ddepth, 0, 1, ksize=3, scale=scale, delta=delta, borderType=cv.BORDER_DEFAULT)
abs_grad_x = cv.convertScaleAbs(grad_x)
abs_grad_y = cv.convertScaleAbs(grad_y)
grad = cv.addWeighted(abs_grad_x, 0.5, abs_grad_y, 0.5, 0)
cv.imshow(window_name, grad)
cv.waitKey(0)
return 0
if __name__ == "__main__":
main(sys.argv[1:])

## Explanation

#### Declare variables

// First we declare the variables we are going to use
Mat image,src, src_gray;
Mat grad;
const String window_name = "Sobel Demo - Simple Edge Detector";
int ksize = parser.get<int>("ksize");
int scale = parser.get<int>("scale");
int delta = parser.get<int>("delta");
int ddepth = CV_16S;

#### Load source image

String imageName = parser.get<String>("@input");
// As usual we load our source image (src)
image = imread( imageName, IMREAD_COLOR ); // Load an image
// Check if image is loaded fine
if( image.empty() )
{
printf("Error opening image: %s\n", imageName.c_str());
return 1;
}

#### Reduce noise

// Remove noise by blurring with a Gaussian filter ( kernel size = 3 )
GaussianBlur(image, src, Size(3, 3), 0, 0, BORDER_DEFAULT);

#### Grayscale

// Convert the image to grayscale
cvtColor(src, src_gray, COLOR_BGR2GRAY);

#### Sobel Operator

Mat grad_x, grad_y;
Mat abs_grad_x, abs_grad_y;
Sobel(src_gray, grad_x, ddepth, 1, 0, ksize, scale, delta, BORDER_DEFAULT);
Sobel(src_gray, grad_y, ddepth, 0, 1, ksize, scale, delta, BORDER_DEFAULT);

- We calculate the "derivatives" in x and y directions. For this, we use the function Sobel() as shown below: The function takes the following arguments:

  - src_gray: In our example, the input image. Here it is CV_8U
  - grad_x / grad_y : The output image.
  - ddepth: The depth of the output image. We set it to CV_16S to avoid overflow.
  - x_order: The order of the derivative in x direction.
  - y_order: The order of the derivative in y direction.
  - scale, delta and BORDER_DEFAULT: We use default values.

  Notice that to calculate the gradient in x direction we use: \(x_{order}= 1\) and \(y_{order} = 0\). We do analogously for the y direction.

#### Convert output to a CV_8U image

// converting back to CV_8U
convertScaleAbs(grad_x, abs_grad_x);
convertScaleAbs(grad_y, abs_grad_y);

#### Gradient

addWeighted(abs_grad_x, 0.5, abs_grad_y, 0.5, 0, grad);

We try to approximate the gradient by adding both directional gradients (note that this is not an exact calculation at all! but it is good for our purposes).

#### Show results

imshow(window_name, grad);
char key = (char)waitKey(0);

## Results

1. Here is the output of applying our basic detector to lena.jpg: