| OpenCV 3.4.3 Open Source Computer Vision

ArUco marker detection (aruco module)

ArUco markers are binary square fiducial markers that can be used for camera pose estimation. Their main benefit is that their detection is robust, fast and simple.

The aruco module includes the detection of these types of markers and the tools to employ them for pose estimation and camera calibration.

Also, the ChArUco functionalities combine ArUco markers with traditional chessboards to allow an easy and versatile corner detection. The module also includes the functions to detect ChArUco corners and use them for pose estimation and camera calibration.

- Detection of ArUco Markers

  Compatibility: > OpenCV 3.0

  Author: Sergio Garrido

  Basic detection and pose estimation from single ArUco markers.

- Detection of ArUco Boards

  Compatibility: > OpenCV 3.0

  Author: Sergio Garrido

  Detection and pose estimation using a Board of markers

- Detection of ChArUco Corners

  Compatibility: > OpenCV 3.0

  Author: Sergio Garrido

  Basic detection using ChArUco corners

- Detection of Diamond Markers

  Compatibility: > OpenCV 3.0

  Author: Sergio Garrido

  Detection and pose estimation using ChArUco markers

- Calibration with ArUco and ChArUco

  Compatibility: > OpenCV 3.0

  Author: Sergio Garrido

  Camera Calibration using ArUco and ChArUco boards

- Aruco module FAQ

  Compatibility: > OpenCV 3.0

  Author: Sergio Garrido

  General and useful questions about the aruco module