| OpenCV 3.4.3 Open Source Computer Vision

Modules | Classes | Functions
Image Processing
Core functionality » OpenGL interoperability » CUDA-accelerated Computer Vision

## Modules
| Color space processing
| Histogram Calculation
| Hough Transform
| Feature Detection

## Classes
class | cv::cuda::CannyEdgeDetector
| Base class for Canny Edge Detector. : More...
class | cv::cuda::TemplateMatching
| Base class for Template Matching. : More...

## Functions
void | cv::cuda::bilateralFilter (InputArray src, OutputArray dst, int kernel_size, float sigma_color, float sigma_spatial, int borderMode=BORDER_DEFAULT, Stream &stream=Stream::Null())
| Performs bilateral filtering of passed image. More...
void | cv::cuda::blendLinear (InputArray img1, InputArray img2, InputArray weights1, InputArray weights2, OutputArray result, Stream &stream=Stream::Null())
| Performs linear blending of two images. More...
Ptr< CannyEdgeDetector > | cv::cuda::createCannyEdgeDetector (double low_thresh, double high_thresh, int apperture_size=3, bool L2gradient=false)
| Creates implementation for cuda::CannyEdgeDetector . More...
Ptr< TemplateMatching > | cv::cuda::createTemplateMatching (int srcType, int method, Size user_block_size=Size())
| Creates implementation for cuda::TemplateMatching . More...
void | cv::cuda::meanShiftFiltering (InputArray src, OutputArray dst, int sp, int sr, TermCriteria criteria=TermCriteria(TermCriteria::MAX_ITER+TermCriteria::EPS, 5, 1), Stream &stream=Stream::Null())
| Performs mean-shift filtering for each point of the source image. More...
void | cv::cuda::meanShiftProc (InputArray src, OutputArray dstr, OutputArray dstsp, int sp, int sr, TermCriteria criteria=TermCriteria(TermCriteria::MAX_ITER+TermCriteria::EPS, 5, 1), Stream &stream=Stream::Null())
| Performs a mean-shift procedure and stores information about processed points (their colors and positions) in two images. More...
void | cv::cuda::meanShiftSegmentation (InputArray src, OutputArray dst, int sp, int sr, int minsize, TermCriteria criteria=TermCriteria(TermCriteria::MAX_ITER+TermCriteria::EPS, 5, 1), Stream &stream=Stream::Null())
| Performs a mean-shift segmentation of the source image and eliminates small segments. More...

## Detailed Description

## Function Documentation

## § bilateralFilter()

void cv::cuda::bilateralFilter | ( | InputArray | src,
|  | OutputArray | dst,
|  | int | kernel_size,
|  | float | sigma_color,
|  | float | sigma_spatial,
|  | int | borderMode = `BORDER_DEFAULT`,
|  | Stream & | stream = `Stream::Null()`
| ) |  |

Performs bilateral filtering of passed image.

Parameters

  src | Source image. Supports only (channels != 2 && depth() != CV_8S && depth() != CV_32S && depth() != CV_64F).
  dst | Destination imagwe.
  kernel_size | Kernel window size.
  sigma_color | Filter sigma in the color space.
  sigma_spatial | Filter sigma in the coordinate space.
  borderMode | Border type. See borderInterpolate for details. BORDER_REFLECT101 , BORDER_REPLICATE , BORDER_CONSTANT , BORDER_REFLECT and BORDER_WRAP are supported for now.
  stream | Stream for the asynchronous version.

See also
  bilateralFilter

## § blendLinear()

void cv::cuda::blendLinear | ( | InputArray | img1,
|  | InputArray | img2,
|  | InputArray | weights1,
|  | InputArray | weights2,
|  | OutputArray | result,
|  | Stream & | stream = `Stream::Null()`
| ) |  |

Performs linear blending of two images.

Parameters

  img1 | First image. Supports only CV_8U and CV_32F depth.
  img2 | Second image. Must have the same size and the same type as img1 .
  weights1 | Weights for first image. Must have tha same size as img1 . Supports only CV_32F type.
  weights2 | Weights for second image. Must have tha same size as img2 . Supports only CV_32F type.
  result | Destination image.
  stream | Stream for the asynchronous version.

## § createCannyEdgeDetector()

Ptr<CannyEdgeDetector> cv::cuda::createCannyEdgeDetector | ( | double | low_thresh,
|  | double | high_thresh,
|  | int | apperture_size = `3`,
|  | bool | L2gradient = `false`
| ) |  |

Creates implementation for cuda::CannyEdgeDetector .

Parameters

  low_thresh | First threshold for the hysteresis procedure.
  high_thresh | Second threshold for the hysteresis procedure.
  apperture_size | Aperture size for the Sobel operator.
  L2gradient | Flag indicating whether a more accurate \(L_2\) norm \(=\sqrt{(dI/dx)^2 + (dI/dy)^2}\) should be used to compute the image gradient magnitude ( L2gradient=true ), or a faster default \(L_1\) norm \(=|dI/dx|+|dI/dy|\) is enough ( L2gradient=false ).

## § createTemplateMatching()

Ptr<TemplateMatching> cv::cuda::createTemplateMatching | ( | int | srcType,
|  | int | method,
|  | Size | user_block_size = `Size()`
| ) |  |

Creates implementation for cuda::TemplateMatching .

Parameters

  srcType | Input source type. CV_32F and CV_8U depth images (1..4 channels) are supported for now.
  method | Specifies the way to compare the template with the image.
  user_block_size | You can use field user_block_size to set specific block size. If you leave its default value Size(0,0) then automatic estimation of block size will be used (which is optimized for speed). By varying user_block_size you can reduce memory requirements at the cost of speed.

The following methods are supported for the CV_8U depth images for now:

- CV_TM_SQDIFF
- CV_TM_SQDIFF_NORMED
- CV_TM_CCORR
- CV_TM_CCORR_NORMED
- CV_TM_CCOEFF
- CV_TM_CCOEFF_NORMED

The following methods are supported for the CV_32F images for now:

- CV_TM_SQDIFF
- CV_TM_CCORR

See also
  matchTemplate

## § meanShiftFiltering()

void cv::cuda::meanShiftFiltering | ( | InputArray | src,
|  | OutputArray | dst,
|  | int | sp,
|  | int | sr,
|  | TermCriteria | criteria = `TermCriteria(TermCriteria::MAX_ITER+TermCriteria::EPS, 5, 1)`,
|  | Stream & | stream = `Stream::Null()`
| ) |  |

Performs mean-shift filtering for each point of the source image.

Parameters

  src | Source image. Only CV_8UC4 images are supported for now.
  dst | Destination image containing the color of mapped points. It has the same size and type as src .
  sp | Spatial window radius.
  sr | Color window radius.
  criteria | Termination criteria. See TermCriteria.
  stream | Stream for the asynchronous version.

It maps each point of the source image into another point. As a result, you have a new color and new position of each point.

## § meanShiftProc()

void cv::cuda::meanShiftProc | ( | InputArray | src,
|  | OutputArray | dstr,
|  | OutputArray | dstsp,
|  | int | sp,
|  | int | sr,
|  | TermCriteria | criteria = `TermCriteria(TermCriteria::MAX_ITER+TermCriteria::EPS, 5, 1)`,
|  | Stream & | stream = `Stream::Null()`
| ) |  |

Performs a mean-shift procedure and stores information about processed points (their colors and positions) in two images.

Parameters

  src | Source image. Only CV_8UC4 images are supported for now.
  dstr | Destination image containing the color of mapped points. The size and type is the same as src .
  dstsp | Destination image containing the position of mapped points. The size is the same as src size. The type is CV_16SC2 .
  sp | Spatial window radius.
  sr | Color window radius.
  criteria | Termination criteria. See TermCriteria.
  stream | Stream for the asynchronous version.

See also
  cuda::meanShiftFiltering

## § meanShiftSegmentation()

void cv::cuda::meanShiftSegmentation | ( | InputArray | src,
|  | OutputArray | dst,
|  | int | sp,
|  | int | sr,
|  | int | minsize,
|  | TermCriteria | criteria = `TermCriteria(TermCriteria::MAX_ITER+TermCriteria::EPS, 5, 1)`,
|  | Stream & | stream = `Stream::Null()`
| ) |  |

Performs a mean-shift segmentation of the source image and eliminates small segments.

Parameters

  src | Source image. Only CV_8UC4 images are supported for now.
  dst | Segmented image with the same size and type as src (host memory).
  sp | Spatial window radius.
  sr | Color window radius.
  minsize | Minimum segment size. Smaller segments are merged.
  criteria | Termination criteria. See TermCriteria.
  stream | Stream for the asynchronous version.