| OpenCV 3.4.8 Open Source Computer Vision

Modules | Functions
Extended Image Processing

## Modules
| Structured forests for fast edge detection
| EdgeBoxes
| Filters
| Superpixels
| Image segmentation
| Fast line detector
| Fourier descriptors

## Functions
void | cv::ximgproc::anisotropicDiffusion (InputArray src, OutputArray dst, float alpha, float K, int niters)
| Performs anisotropic diffusian on an image. More...
void | cv::ximgproc::niBlackThreshold (InputArray _src, OutputArray _dst, double maxValue, int type, int blockSize, double k, int binarizationMethod=BINARIZATION_NIBLACK)
| Performs thresholding on input images using Niblack's technique or some of the popular variations it inspired. More...
Matx23d | cv::ximgproc::PeiLinNormalization (InputArray I)
| Calculates an affine transformation that normalize given image using Pei&Lin Normalization. More...
void | cv::ximgproc::PeiLinNormalization (InputArray I, OutputArray T)
void | cv::ximgproc::thinning (InputArray src, OutputArray dst, int thinningType=THINNING_ZHANGSUEN)
| Applies a binary blob thinning operation, to achieve a skeletization of the input image. More...

## Detailed Description

## Function Documentation

## § anisotropicDiffusion()

void cv::ximgproc::anisotropicDiffusion | ( | InputArray | src,
|  | OutputArray | dst,
|  | float | alpha,
|  | float | K,
|  | int | niters
| ) |  |

Python:
| dst | = | cv.ximgproc.anisotropicDiffusion( | src, alpha, K, niters[, dst] | )

`#include <opencv2/ximgproc.hpp>`

Performs anisotropic diffusian on an image.

The function applies Perona-Malik anisotropic diffusion to an image. This is the solution to the partial differential equation:

\[{\frac {\partial I}{\partial t}}={\mathrm {div}}\left(c(x,y,t)\nabla I\right)=\nabla c\cdot \nabla I+c(x,y,t)\Delta I\]

Suggested functions for c(x,y,t) are:

\[c\left(\|\nabla I\|\right)=e^{{-\left(\|\nabla I\|/K\right)^{2}}}\]

or

\[ c\left(\|\nabla I\|\right)={\frac {1}{1+\left({\frac {\|\nabla I\|}{K}}\right)^{2}}} \]

Parameters

  src | Source image with 3 channels.
  dst | Destination image of the same size and the same number of channels as src .
  alpha | The amount of time to step forward by on each iteration (normally, it's between 0 and 1).
  K | sensitivity to the edges
  niters | The number of iterations

## § niBlackThreshold()

void cv::ximgproc::niBlackThreshold | ( | InputArray | _src,
|  | OutputArray | _dst,
|  | double | maxValue,
|  | int | type,
|  | int | blockSize,
|  | double | k,
|  | int | binarizationMethod = `BINARIZATION_NIBLACK`
| ) |  |

Python:
| _dst | = | cv.ximgproc.niBlackThreshold( | _src, maxValue, type, blockSize, k[, _dst[, binarizationMethod]] | )

`#include <opencv2/ximgproc.hpp>`

Performs thresholding on input images using Niblack's technique or some of the popular variations it inspired.

The function transforms a grayscale image to a binary image according to the formulae:

- THRESH_BINARY

  \[dst(x,y) = \fork{\texttt{maxValue}}{if \(src(x,y) > T(x,y)\)}{0}{otherwise}\]

- THRESH_BINARY_INV

  \[dst(x,y) = \fork{0}{if \(src(x,y) > T(x,y)\)}{\texttt{maxValue}}{otherwise}\]

  where \(T(x,y)\) is a threshold calculated individually for each pixel.

The threshold value \(T(x, y)\) is determined based on the binarization method chosen. For classic Niblack, it is the mean minus \( k \) times standard deviation of \(\texttt{blockSize} \times\texttt{blockSize}\) neighborhood of \((x, y)\).

The function can't process the image in-place.

Parameters

  _src | Source 8-bit single-channel image.
  _dst | Destination image of the same size and the same type as src.
  maxValue | Non-zero value assigned to the pixels for which the condition is satisfied, used with the THRESH_BINARY and THRESH_BINARY_INV thresholding types.
  type | Thresholding type, see cv::ThresholdTypes.
  blockSize | Size of a pixel neighborhood that is used to calculate a threshold value for the pixel: 3, 5, 7, and so on.
  k | The user-adjustable parameter used by Niblack and inspired techniques. For Niblack, this is normally a value between 0 and 1 that is multiplied with the standard deviation and subtracted from the mean.
  binarizationMethod | Binarization method to use. By default, Niblack's technique is used. Other techniques can be specified, see cv::ximgproc::LocalBinarizationMethods.

See also
  threshold, adaptiveThreshold

## § PeiLinNormalization() [1/2]

Matx23d cv::ximgproc::PeiLinNormalization | ( | InputArray | I | ) |

Python:
| T | = | cv.ximgproc.PeiLinNormalization( | I[, T] | )

`#include <opencv2/ximgproc/peilin.hpp>`

Calculates an affine transformation that normalize given image using Pei&Lin Normalization.

Assume given image \(I=T(\bar{I})\) where \(\bar{I}\) is a normalized image and \(T\) is an affine transformation distorting this image by translation, rotation, scaling and skew. The function returns an affine transformation matrix corresponding to the transformation \(T^{-1}\) described in [PeiLin95]. For more details about this implementation, please see [PeiLin95] Soo-Chang Pei and Chao-Nan Lin. Image normalization for pattern recognition. Image and Vision Computing, Vol. 13, N.10, pp. 711-723, 1995.

Parameters

  I | Given transformed image.

Returns
  Transformation matrix corresponding to inversed image transformation

## § PeiLinNormalization() [2/2]

void cv::ximgproc::PeiLinNormalization | ( | InputArray | I,
|  | OutputArray | T
| ) |  |

Python:
| T | = | cv.ximgproc.PeiLinNormalization( | I[, T] | )

`#include <opencv2/ximgproc/peilin.hpp>`

This is an overloaded member function, provided for convenience. It differs from the above function only in what argument(s) it accepts.

## § thinning()

void cv::ximgproc::thinning | ( | InputArray | src,
|  | OutputArray | dst,
|  | int | thinningType = `THINNING_ZHANGSUEN`
| ) |  |

Python:
| dst | = | cv.ximgproc.thinning( | src[, dst[, thinningType]] | )

`#include <opencv2/ximgproc.hpp>`

Applies a binary blob thinning operation, to achieve a skeletization of the input image.

The function transforms a binary blob image into a skeletized form using the technique of Zhang-Suen.

Parameters

  src | Source 8-bit single-channel image, containing binary blobs, with blobs having 255 pixel values.
  dst | Destination image of the same size and the same type as src. The function can work in-place.
  thinningType | Value that defines which thinning algorithm should be used. See cv::ximgproc::ThinningTypes