| OpenCV 3.4.8 Open Source Computer Vision

Classes | Functions
Hough Transform
CUDA-accelerated Computer Vision » Image Processing

## Classes
class | cv::cuda::HoughCirclesDetector
| Base class for circles detector algorithm. : More...
class | cv::cuda::HoughLinesDetector
| Base class for lines detector algorithm. : More...
class | cv::cuda::HoughSegmentDetector
| Base class for line segments detector algorithm. : More...

## Functions
Ptr< GeneralizedHoughBallard > | cv::cuda::createGeneralizedHoughBallard ()
| Creates implementation for generalized hough transform from [10] . More...
Ptr< GeneralizedHoughGuil > | cv::cuda::createGeneralizedHoughGuil ()
| Creates implementation for generalized hough transform from [82] . More...
Ptr< HoughCirclesDetector > | cv::cuda::createHoughCirclesDetector (float dp, float minDist, int cannyThreshold, int votesThreshold, int minRadius, int maxRadius, int maxCircles=4096)
| Creates implementation for cuda::HoughCirclesDetector . More...
Ptr< HoughLinesDetector > | cv::cuda::createHoughLinesDetector (float rho, float theta, int threshold, bool doSort=false, int maxLines=4096)
| Creates implementation for cuda::HoughLinesDetector . More...
Ptr< HoughSegmentDetector > | cv::cuda::createHoughSegmentDetector (float rho, float theta, int minLineLength, int maxLineGap, int maxLines=4096)
| Creates implementation for cuda::HoughSegmentDetector . More...

## Detailed Description

## Function Documentation

## § createGeneralizedHoughBallard()

Ptr<GeneralizedHoughBallard> cv::cuda::createGeneralizedHoughBallard | ( |  | ) |

`#include <opencv2/cudaimgproc.hpp>`

Creates implementation for generalized hough transform from [10] .

## § createGeneralizedHoughGuil()

Ptr<GeneralizedHoughGuil> cv::cuda::createGeneralizedHoughGuil | ( |  | ) |

`#include <opencv2/cudaimgproc.hpp>`

Creates implementation for generalized hough transform from [82] .

## § createHoughCirclesDetector()

Ptr<HoughCirclesDetector> cv::cuda::createHoughCirclesDetector | ( | float | dp,
|  | float | minDist,
|  | int | cannyThreshold,
|  | int | votesThreshold,
|  | int | minRadius,
|  | int | maxRadius,
|  | int | maxCircles = `4096`
| ) |  |

`#include <opencv2/cudaimgproc.hpp>`

Creates implementation for cuda::HoughCirclesDetector .

Parameters

  dp | Inverse ratio of the accumulator resolution to the image resolution. For example, if dp=1 , the accumulator has the same resolution as the input image. If dp=2 , the accumulator has half as big width and height.
  minDist | Minimum distance between the centers of the detected circles. If the parameter is too small, multiple neighbor circles may be falsely detected in addition to a true one. If it is too large, some circles may be missed.
  cannyThreshold | The higher threshold of the two passed to Canny edge detector (the lower one is twice smaller).
  votesThreshold | The accumulator threshold for the circle centers at the detection stage. The smaller it is, the more false circles may be detected.
  minRadius | Minimum circle radius.
  maxRadius | Maximum circle radius.
  maxCircles | Maximum number of output circles.

## § createHoughLinesDetector()

Ptr<HoughLinesDetector> cv::cuda::createHoughLinesDetector | ( | float | rho,
|  | float | theta,
|  | int | threshold,
|  | bool | doSort = `false`,
|  | int | maxLines = `4096`
| ) |  |

`#include <opencv2/cudaimgproc.hpp>`

Creates implementation for cuda::HoughLinesDetector .

Parameters

  rho | Distance resolution of the accumulator in pixels.
  theta | Angle resolution of the accumulator in radians.
  threshold | Accumulator threshold parameter. Only those lines are returned that get enough votes ( \(>\texttt{threshold}\) ).
  doSort | Performs lines sort by votes.
  maxLines | Maximum number of output lines.

## § createHoughSegmentDetector()

Ptr<HoughSegmentDetector> cv::cuda::createHoughSegmentDetector | ( | float | rho,
|  | float | theta,
|  | int | minLineLength,
|  | int | maxLineGap,
|  | int | maxLines = `4096`
| ) |  |

`#include <opencv2/cudaimgproc.hpp>`

Creates implementation for cuda::HoughSegmentDetector .

Parameters

  rho | Distance resolution of the accumulator in pixels.
  theta | Angle resolution of the accumulator in radians.
  minLineLength | Minimum line length. Line segments shorter than that are rejected.
  maxLineGap | Maximum allowed gap between points on the same line to link them.
  maxLines | Maximum number of output lines.