| OpenCV 4.3.0 Open Source Computer Vision

Public Member Functions | Public Attributes | List of all members
cv::bioinspired::SegmentationParameters Struct Reference
Biologically inspired vision models and derivated tools

parameter structure that stores the transient events detector setup parameters More...

`#include <opencv2/bioinspired/transientareassegmentationmodule.hpp>`

## Public Member Functions
| SegmentationParameters ()

## Public Attributes
float | contextEnergy_spatialConstant
float | contextEnergy_temporalConstant
| context neighborhood energy filtering parameters : the aim is to get information about the energy on a wide neighborhood area to filtered out local effects More...
float | localEnergy_spatialConstant
| the spatial constant of the first order low pass filter, use it to cut high spatial frequencies (noise or thick contours), unit is pixels, typical value is 5 pixel More...
float | localEnergy_temporalConstant
| the time constant of the first order low pass filter, use it to cut high temporal frequencies (noise or fast motion), unit is frames, typical value is 0.5 frame More...
float | neighborhoodEnergy_spatialConstant
float | neighborhoodEnergy_temporalConstant
| local neighborhood energy filtering parameters : the aim is to get information about the energy neighborhood to perform a center surround energy analysis More...
float | thresholdOFF
float | thresholdON

## Detailed Description

parameter structure that stores the transient events detector setup parameters

## Constructor & Destructor Documentation

## ◆ SegmentationParameters()

cv::bioinspired::SegmentationParameters::SegmentationParameters | ( |  | ) |
| inline

## Member Data Documentation

## ◆ contextEnergy_spatialConstant

float cv::bioinspired::SegmentationParameters::contextEnergy_spatialConstant

## ◆ contextEnergy_temporalConstant

float cv::bioinspired::SegmentationParameters::contextEnergy_temporalConstant

context neighborhood energy filtering parameters : the aim is to get information about the energy on a wide neighborhood area to filtered out local effects

## ◆ localEnergy_spatialConstant

float cv::bioinspired::SegmentationParameters::localEnergy_spatialConstant

the spatial constant of the first order low pass filter, use it to cut high spatial frequencies (noise or thick contours), unit is pixels, typical value is 5 pixel

## ◆ localEnergy_temporalConstant

float cv::bioinspired::SegmentationParameters::localEnergy_temporalConstant

the time constant of the first order low pass filter, use it to cut high temporal frequencies (noise or fast motion), unit is frames, typical value is 0.5 frame

## ◆ neighborhoodEnergy_spatialConstant

float cv::bioinspired::SegmentationParameters::neighborhoodEnergy_spatialConstant

## ◆ neighborhoodEnergy_temporalConstant

float cv::bioinspired::SegmentationParameters::neighborhoodEnergy_temporalConstant

local neighborhood energy filtering parameters : the aim is to get information about the energy neighborhood to perform a center surround energy analysis

## ◆ thresholdOFF

float cv::bioinspired::SegmentationParameters::thresholdOFF

## ◆ thresholdON

float cv::bioinspired::SegmentationParameters::thresholdON

The documentation for this struct was generated from the following file:

- opencv2/bioinspired/transientareassegmentationmodule.hpp